**Bài lap = tiếng anh**

LAN4 188.88.128.0/24 255.255.255.0

LAN2 188.88.129.0/24 255.255.255.0

LOOPBACK3 188.88.130.0/24 255.255.255.0

LAN1 188.88.131.0/25 255.255.255.128 2001::/64

WAN1 188.88.131.128/30 255.255.255.252 2000:DB1::/64

WAN2 188.88.131.132/30 255.255.255.252 2000:DB2::/64

LAN3 2002::/64

DNS

200.1.1.0/24

2003::0/64

enable

config ter

hostname SITE1

banner motd #This is BKACAD-SITE1-GATEWAY#

interface f0/0

description Connect to LAN1

ip address 188.88.131.1 255.255.255.128

ipv6 address 2001::1/64

no shutdown

exit

interface f0/1

description Connect to LAN2

ip address 188.88.129.1 255.255.255.0

no shutdown

exit

interface s0/0 /0

description Connect to Internet

ip address 188.88.131.129 255.255.255.252

ipv6 address 2000:DB1::1/64

no shutdown

exit

----------------

enable

config ter

hostname SITE2

banner motd #This is BKACAD-SITE2-GATEWAY#

interface f0/0

description Connect to LAN3

ipv6 address 2002::1/64

no shutdown

exit

interface f0/1

description Connect to LAN4

ip address 188.88.128.1 255.255.255.0

no shutdown

exit

interface Serial0/0/0

description Connect to Internet

ip address 188.88.131.133 255.255.255.252

ipv6 address 2000:DB2::1/64

no shutdown

exit

interface loopback3

ip address 188.88.130.1 255.255.255.0

no shutdown

exit

--------

enable

conf ter

line console 0

password cisco@console

login

line vty 0 4

password cisco@vty

login

enable secret cisco@enable

**ĐỀ 1**

NHANH 3 190.19.0.0/23 255.255.254.0 2021:A3::/64

NHANH 1 190.19.2.0/24 255.255.255.0 2021:A1::/64

NHANH 2 190.19.3.0/25 255.255.255.128 2021:A2::/64

LOOKPACK 3 n=3 190.19.3.128/29 255.255.255.248

WAN2 190.19.3.136/29 255.255.255.248 2021:FEFE::/64

WAN1 190.19.3.144/30 255.255.255.252 2021:CAFE::/64

enable

conf ter

hostname HAIPHONG

banner motd #Connect: WAN 1#

interface g0/0

description Connect to Nhanh 1

ip address 190.19.2.1 255.255.255.0

ipv6 address 2021:A1::1/64

no shutdown

exit

interface s0/3/0

description Connect to WAN1

ip address 190.19.3.145 255.255.255.252

ipv6 address 2021:CAFE::1/64

no shutdown

exit

-------------------------

enable

conf ter

hostname HANOI

banner motd #Connect: WAN 1 - WAN 2#

interface g0/0

description Connect to Nhanh 2

ip address 190.19.3.1 255.255.255.128

ipv6 address 2021:A2::1/64

no shutdown

exit

interface s0/1/0

description Connect to WAN1

ip address 190.19.3.146 255.255.255.252

ipv6 address 2021:CAFE::2/64

no shutdown

exit

interface s0/1/1

description Connect to WAN2

ip address 190.19.3.137 255.255.255.248

ipv6 address 2021:FEFE::1/64

no shutdown

exit

interface loopback3

ip address 190.19.3.128 255.255.255.248

no shutdown

exit

------------

enable

conf ter

hostname HOABINH

banner motd #Connect: WAN 2#

interface g0/0

description Connect to Nhanh 3

ip address 190.19.0.1 255.255.254.0

ipv6 address 2021:A3::1/64

no shutdown

exit

interface s0/1/1

description Connect to WAN 2

ip address 190.19.3.138 255.255.255.248

ipv6 address 2021:FEFE::2/64

no shutdown

exit

---------------

enable

conf ter

line console 0

password Console@Cisco

login

line vty 6 12

password Vty@Cisco

login

enable secret Cisco@Enable

**BÀI LỚP 23**

enable

config ter

hostname DUONGTANH\_45\_0

interface f0/0

ip address 172.16.0.1 255.255.0.0

no shutdown

exit

interface f1/0

ip address 203.16.30.129 255.255.255.192

no shutdown

exit

interface f0/1

ip address 100.0.0.1 255.0.0.0

no shutdown

exit

enable

config ter

ip dhcp pool LAN1

network 172.16.0.0 255.255.0.0

default-router 172.16.0.1

DNS-SERVER 8.8.8.8

router rip

version 1

network 192.168.0.0

network

-------------

enable

config ter

hostname DUONGTANH\_45\_1

interface f1/0

ip address 192.168.0.1 255.255.255.0

no shutdown

exit

interface f0/1

ip address 203.16.30.130 255.255.255.192

no shutdown

exit

interface f0/0

ip address 200.0.0.2 255.255.0.0

no shutdown

exit

enable

config ter

ip dhcp pool LAN2

network 192.168.0.0 255.255.255.0

default-router 192.168.0.1

DNS-SERVER 8.8.8.8

----------

enable

config ter

hostname DUONGTANH\_45\_2

interface f1/0

ip address 150.1.192.1 255.255.224.0

no shutdown

exit

interface f0/0

ip address 100.0.0.2 255.0.0.0

no shutdown

exit

interface f0/1

ip address 200.0.0.1 255.255.0.0

no shutdown

exit

enable

config ter

ip dhcp pool LAN3

network 150.1.192.0 255.255.224.0

default-router 150.1.192.1

DNS-SERVER 8.8.8.8